# Module: cisco
# Docs: https://www.elastic.co/guide/en/beats/filebeat/7.5/filebeat-module-cisco.html

- module: cisco
  asa:
    enabled: true

    # Set which input to use between syslog (default) or file.
    #var.input: syslog

    # The interface to listen to UDP based syslog traffic. Defaults to
    # localhost. Set to 0.0.0.0 to bind to all available interfaces.
    #var.syslog_host: localhost

    # The UDP port to listen for syslog traffic. Defaults to 9001.
    #var.syslog_port: 9001

    # Set the log level from 1 (alerts only) to 7 (include all messages).
    # Messages with a log level higher than the specified will be dropped.
    # See https://www.cisco.com/c/en/us/td/docs/security/asa/syslog/b_syslog/syslogs-sev-level.html
    #var.log_level: 7

  ftd:
    enabled: true

    # Set which input to use between syslog (default) or file.
    #var.input: syslog

    # The interface to listen to UDP based syslog traffic. Defaults to
    # localhost. Set to 0.0.0.0 to bind to all available interfaces.
    #var.syslog_host: localhost

    # The UDP port to listen for syslog traffic. Defaults to 9003.
    #var.syslog_port: 9003

    # Set the log level from 1 (alerts only) to 7 (include all messages).
    # Messages with a log level higher than the specified will be dropped.
    # See https://www.cisco.com/c/en/us/td/docs/security/firepower/Syslogs/b_fptd_syslog_guide/syslogs-sev-level.html
    #var.log_level: 7

  ios:
    enabled: true

    # Set which input to use between syslog (default) or file.
    #var.input: syslog

    # The interface to listen to UDP based syslog traffic. Defaults to
    # localhost. Set to 0.0.0.0 to bind to all available interfaces.
    #var.syslog_host: localhost

    # The UDP port to listen for syslog traffic. Defaults to 9002.
    #var.syslog_port: 9002

    # Set custom paths for the log files when using file input. If left empty,
    # Filebeat will choose the paths depending on your OS.
    #var.paths:
