# Module: cisco
# Docs: https://www.elastic.co/guide/en/beats/filebeat/8.3/filebeat-module-cisco.html

- module: cisco
  asa:
    enabled: false

    # Set which input to use between udp (default), tcp or file.
    #var.input: udp

    # The interface to listen to udp or tcp syslog traffic. Defaults to
    # localhost. Set to 0.0.0.0 to bind to all available interfaces.
    #var.syslog_host: localhost

    # The port to listen for udp or tcp syslog traffic. Defaults to 9001.
    #var.syslog_port: 9001

    # With tcp input, set the optional tls configuration:
    #var.ssl:
    #  enabled: true
    #  certificate: /path/to/cert.pem
    #  key: /path/to/privatekey.pem
    #  key_passphrase: 'password for my key'

    # Set the log level from 1 (alerts only) to 7 (include all messages).
    # Messages with a log level higher than the specified will be dropped.
    # See https://www.cisco.com/c/en/us/td/docs/security/asa/syslog/b_syslog/syslogs-sev-level.html
    #var.log_level: 7

    # Set internal security zones. used to override parsed network.direction
    # based on zone egress and ingress
    #var.internal_zones: [ "Internal" ]

    # Set external security zones. used to override parsed network.direction
    # based on zone egress and ingress
    #var.external_zones: [ "External" ]

  ftd:
    enabled: false

    # Set which input to use between udp (default), tcp or file.
    #var.input: udp

    # The interface to listen to tcp or udp syslog traffic. Defaults to
    # localhost. Set to 0.0.0.0 to bind to all available interfaces.
    #var.syslog_host: localhost

    # The UDP port to listen for tcp or udp syslog traffic. Defaults to 9003.
    #var.syslog_port: 9003

    # With tcp input, set the optional tls configuration:
    #var.ssl:
    #  enabled: true
    #  certificate: /path/to/cert.pem
    #  key: /path/to/privatekey.pem
    #  key_passphrase: 'password for my key'

    # Set the log level from 1 (alerts only) to 7 (include all messages).
    # Messages with a log level higher than the specified will be dropped.
    # See https://www.cisco.com/c/en/us/td/docs/security/firepower/Syslogs/b_fptd_syslog_guide/syslogs-sev-level.html
    #var.log_level: 7

    # Set internal security zones. used to override parsed network.direction
    # based on zone egress and ingress
    #var.internal_zones: [ "Internal" ]

    # Set external security zones. used to override parsed network.direction
    # based on zone egress and ingress
    #var.external_zones: [ "External" ]

  ios:
    enabled: false

    # Set which input to use between syslog (default) or file.
    #var.input: syslog

    # The interface to listen to syslog traffic. Defaults to
    # localhost. Set to 0.0.0.0 to bind to all available interfaces.
    #var.syslog_host: localhost

    # The port to listen on for syslog traffic. Defaults to 9002.
    #var.syslog_port: 9002

    # Set which protocol to use between udp (default) or tcp.
    #var.syslog_protocol: udp

    # Set custom paths for the log files when using file input. If left empty,
    # Filebeat will choose the paths depending on your OS.
    #var.paths:

  nexus:
    enabled: false

    # Set which input to use between udp (default), tcp or file.
    # var.input: udp
    # var.syslog_host: localhost
    # var.syslog_port: 9506

    # Set paths for the log files when file input is used.
    # var.paths:

    # Toggle output of non-ECS fields (default true).
    # var.rsa_fields: true

    # Set custom timezone offset.
    # "local" (default) for system timezone.
    # "+02:00" for GMT+02:00
    # var.tz_offset: local

  meraki:
    enabled: false

    # Set which input to use between udp (default), tcp or file.
    # var.input: udp
    # var.syslog_host: localhost
    # var.syslog_port: 9525

    # Set paths for the log files when file input is used.
    # var.paths:

    # Toggle output of non-ECS fields (default true).
    # var.rsa_fields: true

    # Set custom timezone offset.
    # "local" (default) for system timezone.
    # "+02:00" for GMT+02:00
    # var.tz_offset: local

  umbrella:
    enabled: false

    #var.input: aws-s3
    # AWS SQS queue url
    #var.queue_url: https://sqs.us-east-1.amazonaws.com/ID/CiscoQueue
    # Access ID to authenticate with the S3 input
    #var.access_key_id: 123456
    # Access key to authenticate with the S3 input
    #var.secret_access_key: PASSWORD
    # The duration that the received messages are hidden from ReceiveMessage request
    #var.visibility_timeout: 300s
    # Maximum duration before AWS API request will be interrupted
    #var.api_timeout: 120s

  amp:
    enabled: false

    # Set which input to use between httpjson (default) or file.
    #var.input: httpjson

    # The API URL
    #var.url: https://api.amp.cisco.com/v1/events
    # The client ID used as a username for the API requests.
    #var.client_id:
    # The API key related to the client ID.
    #var.api_key:
    # How far to look back the first time the module is started. Expects an amount of hours.
    #var.first_interval: 24h
    # Overriding the default request timeout, optional.
    #var.request_timeout: 60s
